Item number Description

Autrosafe 4 module

|  |  |
| --- | --- |
| BSS-310A | Power Module, 24Vdc & 5Vdc 0,9 Amp for I/O modules |
| BSD-310 | Detector loop module 1 loop 127 units(Rmax-50) m=140mA |
| BSD-310/N | Detector loop module 1 loop 127 units(Rmax-50) for Exn/IIBT4 |
| BSJ-310 | Control output module, 8 x open collector NO, max 100mA |
| BSE-310 | Remote Contr. Input Module, 4 mon. dig. Inputs |
| BSE-320 | Remote Contr. Input Module, 8 mon. dig. Inputs |
| BSL-310 | Communications module, RS-232 Galv. isol. |
| BPS-410 | BPS-410 PSU 24V/10A BOXED |

Smoke Detector

|  |  |  |
| --- | --- | --- |
| BHH-200 | Optical Smoke Detector head, IP44D |  |
| BHH-300 | Optical Smoke Detector head, IP44D SV |  |
| BHH-500 | Optical Smoke Detector head, Special Coated | IP44D SV |
| BHH-500/N | Optical Smoke Detector head, Exn/IIBT4, IP44D SV Zone2 | |
| BHH-500/Ex | Optical Smoke Detector head, Exi/IICT5, IP44D SV | |

Heat Detector

|  |  |
| --- | --- |
| BDH-200 | Heat detector head, (Config. 56-88 deg.C), IP44D |
| BDH-500 | Heat Detector head, (Config. 56-88 deg.C) IP 44D SV |
| BDH-500/N | Heat detector head, (Config. 56-88 deg.C), Exn/IIBT4 IP44D SV Z-2 |
| BDH-500/EX | Heat detector head, (Config. 56-88 deg.C) Exi/IICT5 IP44D SV Z-1 |
| BD-501 | Heat detector, (Config. 56-88 deg.C) SV IP 56 |
| BD-501/N | Heat detector, (Config. 56-88 deg.C) SV Exn/IIBT4 IP 56 Z-2 |
| BD-501/Ex | Heat detector, (Config. 56-88 deg.C) SV Exi/IICT5 IP 56 Z-1 |

Flame Detector

BG-201 Autroflame Dual IR Loop powered. IP67

Multi Detector

|  |  |
| --- | --- |
| BHH-220 | Multi Sensor head, optical/Heat, IP44D |
| BHH-320 | Multi Sensor head, optical/Heat, IP44D SV |
| BHH-520 | Multi Sensor head, Smoke/Heat, Special Coated IP44D SV |
| BHH-520/Ex | Multi Sensor head, Smoke/Heat, Exi/IICT5 S.C. IP44D SV |
| BHH-520/N | Multi Sensor head, optical/Heat, Exn/IIBT4, S.C. IP44D SV Zone2 |

Detector Base

|  |  |
| --- | --- |
| BWA-100 | Detector Socket (BDH/BHH detector heads) |
| BWP-100/20 | Conduit box w/M20(6-12mm) glands(for BWA-xxx) 2 glands |

Manual Call Point

|  |  |
| --- | --- |
| BF-300V2 | Manual call point, IP43 SV w/glass "push here"(BFG-3). |
| BF-510WP-H | Manual call point, IP52 SV w/glass "push here"(BFG-3). |
| 6571-011.1922 | Cable gland M20x1,5, for BF500WP+BF500V2Ex |
| 6531-006.1920 | Gland back nut M20x1,5, for BF500WP+BF500V2Ex |
| 4860-011.0100 | Front cover, for BF-500WP-H (IP55) |
| BF-501 | Manual call point, M20 glands IP67 SV |
| BF-501/N | Multi Sensor head, optical/Heat, Exn/IIBT4, S.C. IP44D SV Zone2 |
| BF-502 | Manual call point, M20 glands IP66 SV |
| BF-502/N | Manual call point, M20 glands Exn/IIBT4 IP66 SV |

|  |  |
| --- | --- |
| BF-501/Ex | Manual call point, M20 glands Exi/IICT5 IP67 SV |
| BF-502/Ex | Manual call point, M20 glands Exi/IICT5 IP66 SV |
| BFG-3/GB | Glass for manual call points - English |

Loop Interface

|  |  |
| --- | --- |
| BZ-500 | Ex interface Unit, ExiaIIC, 1 Branch, < 20 det.( sep. 24V). Rev3 |
| BW-200/GB | Disconnect unit timer, local (With Buttons) IP66 |
| BN-300 | Loop Interface Input unit, 1 mon.digital input, SV |
| BN-320/2 | Std Door contr.Interf. unit 2 Dig.mon.inp(Sw.< 100m )/1 pot.fr.outp. |

Alarm Device

BBR-52 LP Smart Buzzer, for socket mounting 80dB/1m 8mA

Test tool

|  |  |
| --- | --- |
| WBJ-5/04 | Test gas bottle, SOLO A3-016 |
| WBJ-5/01 | Smoke det. test unit, SOLO 330 - NB! Pole 5/02 or 5/05 |
| WBJ-5/02 | Telescopic Pole (fibre glass), 1,26-4,5m SOLO 100 |

Autroprime Main Board

|  |  |
| --- | --- |
| BSD-200A/PACK | Loop Board Kit (2 loops) for Autroprime 2 |
| BSA-200A | Main Board for Autroprime 2 - 2 Loops |